gdkPixbufApplyEmbeddedOrientation {RGtk2} | R Documentation

## gdkPixbufApplyEmbeddedOrientation

### Description

Takes an existing pixbuf and checks for the presence of an associated "orientation" option, which may be provided by the jpeg loader (which reads the exif orientation tag) or the tiff loader (which reads the tiff orientation tag, and compensates it for the partial transforms performed by libtiff). If an orientation option/tag is present, the appropriate transform will be performed so that the pixbuf is oriented correctly.

### Usage

    gdkPixbufApplyEmbeddedOrientation(object)

### Arguments

``object`` | A `GdkPixbuf`.

### Details

Since 2.12

### Value

[`GdkPixbuf`] A newly-created pixbuf, or a reference to the input pixbuf (with an increased reference count).

### Author(s)

Derived by RGtkGen from GTK+ documentation

[Package RGtk2 version 2.20.40 Index]